§%1	#AIL# 1399243 78 21 A 01 74 STANDARD2.CTG #F#	23/01/03
§%2

Reference:	.


Version:

Supplier:	Telemecanique

AS-i Profil:

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0:
P1:
P2:
P3:
§%3	f1
§%4	0
§%5	0
§%6	.
§%7
§%8
§%9
§%10
§%11
§%12
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XAL-S2001

2 spring return flush pushbuttons
      Pushbutton "I" (N/O contact) white diam. 22.
      Pushbutton "0" (N/C contact) black diam. 22.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
D0:"I" unoper.=0 ct.open./"I" oper.=1 ct.closed
D1:"0" oper.=0 ct.open./"0" unoper.=1 ct.closed
D2:
D3:

Outputs:
D0:
D1:
D2: Unused
D3: Unused

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	9
§%6	XAL-S2001
§%7	Pushbutton I White - 0 Black
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XAL-S2002

2 spring return flush pushbuttons
      Pushbutton "I" (N/O contact) green diam. 22.
      Pushbutton "0" (N/C contact) red diam. 22.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
D0:"I" unoper.=0 ct.open./"I" oper.=1 ct.closed
D1:"0" oper.=0 ct.open./"0" unoper.=1 ct.closed
D2:
D3:

Outputs:
D0:
D1:
D2: Unused
D3: Unused

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	10
§%6	XAL-S2002
§%7	Pushbutton I Green - 0 Red
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XAL-S2003

2 spring return illuminated flush pushbuttons
      Pushbutton "I" (N/O contact) green diam. 22.
      Pushbutton "0" (N/C contact) red diam. 22.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
D0:"I" unoper.=0 ct.open./"I" oper.=1 ct.closed
D1:"0" oper.=0 ct.open./"0" unoper.=1 ct.closed
D2:
D3:

Outputs:
D0:
D1:
D2: Green indicator : off = 0 / illuminated = 1
D3: Red indicator :   off = 0 / illuminated = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	11
§%6	XAL-S2003
§%7	Pushbutton I Green - 0 Red Led
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XAL-SZ1

2I/2O interface for control and signaling units
No control of the signaling mode.
Inputs for 2 discrete N/O or N/C contacts 24V 5mA.
Outputs for 2 LED indicators 24V 20mA.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
D0:Button 1 : cont.opened = 0 / cont.closed = 1
D1:Button 2 : cont.opened = 0 / cont.closed = 1
D2:
D3:

Outputs:
Only for DEL indicators.
D0:
D1:
D2:20 mA 24Vdc Indic1 : OFF = 0 / ON = 1
D3:20 mA 24Vdc Indic2 : OFF = 0 / ON = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	30
§%6	XAL-SZ1
§%7	2I/2O interface
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	APE1FASI1

Telefast SB2   AS-Interface 4 inputs - 4 outputs
for TEGO DIAL.
Inputs PNP 24Vdc powered from the bus.
Outputs 24VDC-1A solid-state. IP20

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc powered via the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Outputs 24VDC-1A solid-state
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2: O-3 Output actuator 3
D3: O-4 Output actuator 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	52
§%6	APE1FASI1
§%7	ASi TEGO DIAL interface 4I/4O
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ZB2-BZS2@

@ = V vertical mounting    @ = H horizontal mounting
4I/4O interface for control and signaling units
for printed circuits boards.
No control of the signaling mode.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
D0:Button 1 : cont.opened = 0 / cont.closed = 1
D1:Button 2 : cont.opened = 0 / cont.closed = 1
D2:Button 3 : cont.opened = 0 / cont.closed = 1
D3:Button 4 : cont.opened = 0 / cont.closed = 1

Outputs:
 Fallback = 0 by watchdog
D0:60 mA 24Vdc Indic.1 : Off = 0 / On = 1
D1:60 mA 24Vdc Indic.2 : Off = 0 / On = 1
D2:60 mA 24Vdc Indic.3 : Off = 0 / On = 1
D3:60 mA 24Vdc Indic.4 : Off = 0 / On = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	29
§%6	ZB2-BZS2@
§%7	4I4O interf PCB steady light
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17	0
§%18	0
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XBTZA994

Interface for MAGELIS HMI units.
Suitable for models XBTH, XBTM, and XBTP.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
Key    Fx:1 2 3 4 5 6 7 8 9 10 11 12  Ent. Nothing
D0 -----> 1 0 1 0 1 0 1 0 1  0  1  0   1     1
D1 -----> 0 1 1 0 0 1 1 0 0  1  1  0   0     1
D2 -----> 0 0 0 1 1 1 1 0 0  0  0  1   1     1
D3 -----> 0 0 0 0 0 0 0 1 1  1  1  1   1     1
Hexa:     1 2 3 4 5 6 7 8 9  A  B  C   D     F

Outputs:
Pages and alarms selection by coding
D0: Coding
D1: Coding
D2: Coding
D3: Coding

Parameters:
Pages and alarms selection by coding
P0: Coding
P1: Coding
P2: Coding
P3: Coding
§%3	f1
§%4	7
§%5	53
§%6	XBTZA994
§%7	ASi XBT (Magelis) interface
§%8	7.F.F.F
§%9	# Coding
§%10	# Coding
§%11	# Coding
§%12	# Coding
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XBZS43

4I/4O  Interface for HARMONY control and
signaling units.
No control of the signaling mode.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:Button 1 : cont.opened = 0 / cont.closed = 1
D1:Button 2 : cont.opened = 0 / cont.closed = 1
D2:Button 3 : cont.opened = 0 / cont.closed = 1
D3:Button 4 : cont.opened = 0 / cont.closed = 1

Outputs:
 Fallback = 0 by watchdog
D0:20 mA 24Vdc Indic.1 : Off = 0 / On = 1
D1:20 mA 24Vdc Indic.2 : Off = 0 / On = 1
D2:20 mA 24Vdc Indic.3 : Off = 0 / On = 1
D3:20 mA 24Vdc Indic.4 : Off = 0 / On = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	7
§%5	55
§%6	XBZS43
§%7	4I/4O HARMONY adap stead light
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XBZS44

4I/4O  Interface for HARMONY control and
signaling units.
Parameters permit to control the signaling mode.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:Button 1 : cont.opened = 0 / cont.closed = 1
D1:Button 2 : cont.opened = 0 / cont.closed = 1
D2:Button 3 : cont.opened = 0 / cont.closed = 1
D3:Button 4 : cont.opened = 0 / cont.closed = 1

Outputs:
 Fallback = 0 by watchdog
D0:20 mA 24Vdc Indic.1 : Off = 0 / On = 1
D1:20 mA 24Vdc Indic.2 : Off = 0 / On = 1
D2:20 mA 24Vdc Indic.3 : Off = 0 / On = 1
D3:20 mA 24Vdc Indic.4 : Off = 0 / On = 1

Parameters:
P0:Indic.1: flashing = 0 / steady = 1
P1:Indic.2: flashing = 0 / steady = 1
P2:Indic.3: flashing = 0 / steady = 1
P3:Indic.4: flashing = 0 / steady = 1
§%3	f1
§%4	7
§%5	14
§%6	XBZS44
§%7	4I/4O HARMONY adap flash light
§%8	7.F.F.F
§%9	I1 Flash/Stead
§%10	I2 Flash/Stead
§%11	I3 Flash/Stead
§%12	I4 Flash/Stead
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ZB2-BZS1@

@ = V vertical mounting    @ = H horizontal mounting
4I/4O interface for control and signaling units
for printed circuits boards. Parameters permit
to control the signaling mode.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:Button 1 : cont.opened = 0 / cont.closed = 1
D1:Button 2 : cont.opened = 0 / cont.closed = 1
D2:Button 3 : cont.opened = 0 / cont.closed = 1
D3:Button 4 : cont.opened = 0 / cont.closed = 1

Outputs:
 Fallback = 0 by watchdog
D0:60 mA 24Vdc Indic.1 : Off = 0 / On = 1
D1:60 mA 24Vdc Indic.2 : Off = 0 / On = 1
D2:60 mA 24Vdc Indic.3 : Off = 0 / On = 1
D3:60 mA 24Vdc Indic.4 : Off = 0 / On = 1

Parameters:
P0:Indic.1: flashing = 0 / steady = 1
P1:Indic.2: flashing = 0 / steady = 1
P2:Indic.3: flashing = 0 / steady = 1
P3:Indic.4: flashing = 0 / steady = 1
§%3	f1
§%4	7
§%5	28
§%6	ZB2-BZS1@
§%7	4I4O interf PCB flashing light
§%8	7.F.F.F
§%9	I1 Flash/Stead
§%10	I2 Flash/Stead
§%11	I3 Flash/Stead
§%12	I4 Flash/Stead
§%13	1
§%14	1
§%15	1
§%16	1
§%17	0
§%18	0
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XVBC21A

Adaptator unit for illuminated indicator banks
XVB = MAXIMO.
This adaptator must be the lowest unit on the stack.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Status unit 1 : 1 = "OK", 0 = "NOK"
D1: Status unit 2 : 1 = "OK", 0 = "NOK"
D2: Status unit 3 : 1 = "OK", 0 = "NOK"
D3: Status unit 4 : 1 = "OK", 0 = "NOK"

Outputs:
Fallback = 0 by watchdog
D0: Unit 1 : "Off" = 0 / "On" = 1
D1: Unit 2 : "Off" = 0 / "On" = 1
D2: Unit 3 : "Off" = 0 / "On" = 1
D3: Unit 4 : "Off" = 0 / "On" = 1

Parameters:
P0:Unit 1: flashing = 0 / continuous = 1
P1:Unit 2: flashing = 0 / continuous = 1
P2:Unit 3: flashing = 0 / continuous = 1
P3:Unit 4: flashing = 0 / continuous = 1
§%3	f1
§%4	6
§%5	50
§%6	XVBC21A
§%7	Illuminated indicator bank XVB
§%8	7.F.F.F
§%9	Unit 1 flashing
§%10	Unit 2 flashing
§%11	Unit 3 flashing
§%12	Unit 4 flashing
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XVA-S102

Adaptator unit for illuminated indicator banks
XVA.
This adaptator must be the lowest unit on the stack.

Version:

Supplier:	Telemecanique

AS-i Profil:	8.F.F.F

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Fallback = 0 by watchdog. Output relay.
D0: Unit 1 : "Off" = 0 / "On" = 1
D1: Unit 2 : "Off" = 0 / "On" = 1
D2: Unit 3 : "Off" = 0 / "On" = 1
D3: Unit 4 : "Off" = 0 / "On" = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	6
§%5	27
§%6	XVA-S102
§%7	Illuminated indicator bank XVA
§%8	8.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XS1-M30AS101

Inductive proximity sensor flush mountable in
metal.  Cylindrical type, M30 x 1,5 threaded, form A
Range = 10 mm.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0:Signal :  "Off" = 0 / Signal "On" = 1
D1:Warning : "On" = 0 / Alarme "Off" = 1
D2:Availibility : Not available = 0/Available = 1
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Diag : Flash "On" = 0 / Flash "Off" = 1
§%3	f1
§%4	11
§%5	34
§%6	XS1-M30AS101
§%7	Ind. prox sens cyl flush 10 mm
§%8	1.1.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Flash On/Off
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XS7-C40AS101

Inductive proximity sensor flush mountable in metal.
Block type form C, plug in body.
5 positions turret head.
Range = 15 mm.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0:Signal :  "Off" = 0 / "On" = 1
D1:Warning : "On" = 0 / "Off" = 1
D2:Availibility : Not available = 0/Available = 1
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Diag : Flash "On" = 0 / Flash "Off" = 1
§%3	f1
§%4	11
§%5	12
§%6	XS7-C40AS101
§%7	Ind. prox. sensor flush 15 mm.
§%8	1.1.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Flash On/Off
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XS8-C40AS101

Inductive proximity sensor non flush mountable in
metal.  Block type form C, plug in body.
5 positions turret head.
Range = 20 mm.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0:Signal :  "Off" = 0 / Signal "On" = 1
D1:Warning : "On" = 0 / Alarme "Off" = 1
D2:Availibility : Not available = 0/Available = 1
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Diag : Flash "On" = 0 / Flash "Off" = 1
§%3	f1
§%4	11
§%5	13
§%6	XS8-C40AS101
§%7	Ind. prox sens non flush 20 mm
§%8	1.1.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Flash On/Off
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME4I

Interface 4 inputs IP67  standard addressing.
Connection to  AS-Interface bus via IDC
4 sensor inputs powered by the bus 200 mA max
Infrared address programming.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	3
§%5	74
§%6	ASIME4I
§%7	Module  4I standard addr.
§%8	0.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME4IE

Interface 4 inputs IP67 extended addressing.
Connection to AS-Interface via IDC
4 sensor inputs powered by the bus 100 mA max
Infrared address programming.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0:
P1:
P2:
P3:
§%3	f1
§%4	3
§%5	98
§%6	ASIME4IE
§%7	Module 4I extended addr.
§%8	0.A.7.0
§%9
§%10
§%11
§%12
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME2I2O

Interface 2I/2O IP67 standard addressing.
Connection to  AS-Interface bus via IDC
2 sensor inputs powered by the bus. Max. 2 solid
state outputs 24V 2A.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2:
D3:

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0:
D1:
D2: O-1 Actuator output 1 D2=0 / 0-1=0
D3: O-2 Actuator output 2 D3=0 / 0-2=0

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	3
§%5	73
§%6	ASIME2I2O
§%7	Interface 2I/2O standard addr
§%8	3.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME4I4O

Interface 4I/4O IP67, standard addressing.
Connection to ASi bus via IDC
4 sensor inputs powered by the bus. Max. 4 solid
state outputs 24V 2A.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Solid state type 24 VDC. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 4
D3: O-4 Actuator output 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	3
§%5	65
§%6	ASIME4I4O
§%7	Module 4I/4O standard addr
§%8	7.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME4O

Interface, 4 outputs, IP67, standard addressing
Connection to AS-Interface bus via IDC
4 solid state outputs 24 VDC PNP 2A max
Infrared address programming

Version:

Supplier:	Telemecanique

AS-i Profil:	8.0.F.E

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Solid state type 24 VDC. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 4
D3: O-4 Actuator output 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	3
§%5	67
§%6	ASIME4O
§%7	Module 4 0utput  standard addr
§%8	8.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIME2I2OE

Interface 2I/2O IP67 extended addressing.
Connection to AS-Interface bus via IDC
2 sensor inputs powered by the bus. Max. 2 solid
state outputs 24V 2A.

Version:

Supplier:	Telemecanique

AS-i Profil:	B.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0:
D1:
D2: Sensor signal
D3: Sensor signal

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0:O-1 Actuator output 1 D0=0 / 0-1=0
D1:O-2 Actuator output 2 D1=0 / 0-2=0
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	3
§%5	97
§%6	ASIME2I2OE
§%7	Interface 2I/2O extended addr
§%8	B.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4IE

Compact IP20 A/B interface for the conn. of
4 sensors to the AS-Interface bus.
PNP type inputs,  24 VDC, powered by the bus.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 200 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	18
§%5	78
§%6	ASI20MT4IE
§%7	A/B interface 4I+J24
§%8	0.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT2I1OTE

Compact standard IP20 A/B interface for the conn of
2 conventional sensors and 1 conventional actuator
 PNP inputs 24 VDC powered by bus.
TRIAC output 230V 2A

Version:

Supplier:	Telemecanique

AS-i Profil:	3.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 200 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2:
D3:

Outputs:
Triac type  Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	18
§%5	82
§%6	ASI20MT2I1OTE
§%7	Interf 2I/1O triac A/B
§%8	3.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I4OR

Compact standard IP20 interface for the conn. of
4 conventional sensors and 4 conventional actuators
 PNP 24VDC inputs powered by bus.
Relay outputs 230V

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 200 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Relay type 230V AC. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: O-4 Actuator output 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	18
§%5	79
§%6	ASI20MT4I4OR
§%7	Std interface 4I/4O relay
§%8	7.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I4OS

Compact standard IP20 interface for the conn. of
4 conventional sensors and 4 conventional actuators
 PNP 24VDC inputs powered by bus.
Solid state outputs 24 VDC

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 200 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: O-4 Actuator output 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	18
§%5	80
§%6	ASI20MT4I4OS
§%7	Std interf 4I/4O solid state
§%8	7.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I4OSA

Compact standard IP20 interface for the conn. of
4 conventional sensors and 4 conventional actuators
 PNP 24VDC inputs isolated from bus.
Solid state outputs 24 VDC

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.E

I/O Configuration:
Inputs:
PNP type  24 VDC isolated from the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: O-4 Actuator output 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	18
§%5	81
§%6	ASI20MT4I4OSA
§%7	Std interf 4Ii/4O solid state
§%8	7.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIMA2VI

Interface with 2 analog inputs 4-20 mA
Resolution on 12 bits
Connection via screw terminals
Infrared address programming

Version:

Supplier:	Telemecanique

AS-i Profil:	7.3.F.D

I/O Configuration:
Inputs:
The analog value is transmitted in triplets
D0: Low order
D1: Medium order
D2: High order
D3: Synchronization bit

Outputs:
Number of triplet to be transmitted
D0: Low order of triplet number
D1: Medium order of triplet number
D2: High order of triplet number
D3: Synchronization bit

Parameters:
P0: Unused
P1: Enable channel 2 1=enabled 0=disabled
P2: Enable overload fault 1=enabled 0=disabled
P3: Unused
§%3	f1
§%4	18
§%5	66
§%6	ASIMA2VI
§%7	Interface 2 ana inputs 4-20mA
§%8	7.3.F.D
§%9	Unused
§%10	Enable channel 2
§%11	Ena overload flt
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIMA2VU

Interface with 2 analog inputs 0-10V
Resolution on 12 bits
Connection via screw terminals
Infrared address programming

Version:

Supplier:	Telemecanique

AS-i Profil:	7.3.F.D

I/O Configuration:
Inputs:
The analog value is transmitted in triplets
D0: Low order
D1: Medium order
D2: High order
D3: Synchronization bit

Outputs:
Number of triplet to be transmitted
D0: Low order of triplet number
D1: Medium order of triplet number
D2: High order of triplet number
D3: Synchronization bit

Parameters:
P0: Unused
P1: Enable channel 2 1=enabled 0=disabled
P2: Enable overload fault 1=enabled 0=disabled
P3: Unused
§%3	f1
§%4	18
§%5	83
§%6	ASIMA2VU
§%7	Interface 2  ana. Inputs 0-10V
§%8	7.3.F.D
§%9	Unused
§%10	Enable channel 2
§%11	Ena overload flt
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I3ORE

Compact IP20 A/B interface for the connection  of
4 conventional sensors and 3 conventional actuators
PNP 24VDC inputs powered by bus.
Relay outputs 230V

Version:

Supplier:	Telemecanique

AS-i Profil:	7.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 170 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Relay type 230V AC. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: Don't use

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Don't use
§%3	f1
§%4	18
§%5	115
§%6	ASI20MT4I3ORE
§%7	A/B interface 4I/3O relay
§%8	7.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Don't use
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I3OSAE

Compact IP20 A/B interface for the connection of
4 conventional sensors and 3 conventional actuators
PNP 24VDC inputs isolated from bus.
Solid state outputs 24 VDC

Version:

Supplier:	Telemecanique

AS-i Profil:	7.A.7.0

I/O Configuration:
Inputs:
PNP type  24 VDC isolated from the bus, 200mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: Don't use

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Don't use
§%3	f1
§%4	18
§%5	113
§%6	ASI20MT4I3OSAE
§%7	A/B interf 4I/3O solid state
§%8	7.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Don't use
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI20MT4I3OSE

Compact IP20 A/B interface for the connection of
4 conventional sensors and 3 conventional actuators
PNP 24VDC inputs powered by bus.
Solid state outputs 24 VDC

Version:

Supplier:	Telemecanique

AS-i Profil:	7.A.7.0

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus 200 mA max
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Solid state type 24Vdc. Fallback = 0 by watchdog
D0: O-1 Actuator output 1
D1: O-2 Actuator output 2
D2: O-3 Actuator output 3
D3: Don't use

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Don't use
§%3	f1
§%4	18
§%5	114
§%6	ASI20MT4I3OSE
§%7	A/B  interf 4I/3O solid state
§%8	7.A.7.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Don't use
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA40D3

Active user module.
Used for the connection of 4 sensors.
PNP 24Vdc inputs
Maximum current for 4 sensors =200 mA.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc
D0: I-1 Sensor signal 1 (pins 4-2)
D1: I-2 Sensor signal 2 (pins 4-2)
D2: I-3 Sensor signal 3 (pins 4-2)
D3: I-4 Sensor signal 4 (pins 4-2)

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	32
§%6	XZ-SDA40D3
§%7	User module 4 I 200 mA
§%8	0.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA22D11

Active user module. Used for the connection of 2
sensors (100 mA max) and 2 actuators (1A max).
Actuators power supply by separate supply via
M12 connector.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.0.F.F

I/O Configuration:
Inputs:
PNP type
D0: I-1 Sensor signal 1 (pins 4-2)
D1: I-2 Sensor signal 2 (pins 4-2)
D2:
D3:

Outputs:
D0:
D1:
D2: O-3 Relay output 24 V DC 1A
D3: O-4 Relay output 24 V DC 1A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	5
§%6	XZ-SDA22D11
§%7	User module  2I/2O relay M12
§%8	3.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA22D12

Active user module. Used for the connection of 2
sensors (100 mA max) and 2 actuators (1A max).
Actuators power supply by separate supply via
its base.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.0.F.F

I/O Configuration:
Inputs:
PNP type
D0: I-1 Sensor signal 1 (pins 4-2)
D1: I-2 Sensor signal 2 (pins 4-2)
D2:
D3:

Outputs:
D0:
D1:
D2: O-3 Relay output 24 V DC 1A
D3: O-4 Relay output 24 V DC 1A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	6
§%6	XZ-SDA22D12
§%7	User module  2I/2O relay base
§%8	3.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA22D32

Active user module. Used for the connection of 2
sensors (100 mA max) and 2 actuators (2A max).
Actuators power supply by separate supply via
its base.

Version:

Supplier:	Telemecanique

AS-i Profil:	3.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc
D0: I-1 Sensor signal 1 (pins 4-2)
D1: I-2 Sensor signal 2 (pins 4-2)
D2:
D3:

Outputs:
Total current by module : 2A. Fallback = 0
D0:
D1:
D2: O-3 Solid-state output 24 V DC 2A
D3: O-4 Solid-state output 24 V DC 2A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	31
§%6	XZ-SDA22D32
§%7	User mod  2I/2O solid sta base
§%8	3.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SCA44D21

Compact module. Used for the connection of 4 sensors
and 4 actuators Inputs PNP 24Vdc Solid-state outputs
24Vdc 2A. Bus and power supply connection by
insulation dispacement connector.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Total current by module : 4A. Fallback = 0
D0: O-1 Solid-state output 24 V DC 2A
D1: O-2 Solid-state output 24 V DC 2A
D2: O-3 Solid-state output 24 V DC 2A
D3: O-4 Solid-state output 24 V DC 2A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	41
§%6	XZ-SCA44D21
§%7	Comp modu  4iI/4O sol sta base
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17	0
§%18	0
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SCA44D22

Compact module. Used for the connection of 4 senors
and 4 actuators Inputs PNP 24Vdc Solid state outputs
24Vdc 2A. Bus and power supply connection by
connector M12

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Total current by module : 4A. Fallback = 0
D0: O-1 Solid-state output 24 V DC 2A
D1: O-2 Solid-state output 24 V DC 2A
D2: O-3 Solid-state output 24 V DC 2A
D3: O-4 Solid-state output 24 V DC 2A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	42
§%6	XZ-SCA44D22
§%7	Comp modu 4iI/4O solid sta M12
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17	0
§%18	0
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA04D21

Active user module.
Used for the connection of 4 actuators.
Actuators power supply by separate supply via
M12 connector.

Version:

Supplier:	Telemecanique

AS-i Profil:	8.0.F.F

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Total current by module : 2A
D0: O-1 Relay output 24 V DC 1A
D1: O-2 Relay output 24 V DC 1A
D2: O-3 Relay output 24 V DC 1A
D3: O-4 Relay output 24 V DC 1A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	7
§%6	XZ-SDA04D21
§%7	User module 4O relay M12
§%8	8.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA04D22

Active user module.
Used for the connection of 4 actuators.
Actuators power supply by separate supply via
its base.

Version:

Supplier:	Telemecanique

AS-i Profil:	8.0.F.F

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Total current by module : 2A.
D0: O-1 Relay output 24 V DC 1A
D1: O-2 Relay output 24 V DC 1A
D2: O-3 Relay output 24 V DC 1A
D3: O-4 Relay output 24 V DC 1A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	8
§%6	XZ-SDA04D22
§%7	User module 4O relay base
§%8	8.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XZ-SDA04D32

Active user module.
Used for the connection of 4 actuators.
Actuators power supply by separate supply via
its base. Solid-state outputs

Version:

Supplier:	Telemecanique

AS-i Profil:	8.0.F.F

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Total current by module : 2A. Fallback = 0
D0: O-1 Solid-state output 24 V DC 2A
D1: O-2 Solid-state output 24 V DC 2A
D2: O-3 Solid-state output 24 V DC 2A
D3: O-4 Solid-state output 24 V DC 2A

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	10
§%5	33
§%6	XZ-SDA04D32
§%7	User module 4O solid stat base
§%8	8.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17	0
§%18	0
§%19	0
§%20	0
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIMMO4I

Mini-module 4 inputs IP67   standard addressing.
Connection to  AS-Interface bus via IDC
4 sensor inputs powered by the bus

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	15
§%5	75
§%6	ASIMMO4I
§%7	Mini-mod 4I std addr IDC
§%8	0.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIMMO4I20

Mini-module 4 inputs IP67 standard addressing.
Connection to Asi bus via M12 2 m extension cable.
4 sensor inputs powered by the bus

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	15
§%5	76
§%6	ASIMMO4I20
§%7	Mini-mod  4I std add M12-2
§%8	0.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASIMMO4I50

Mini-module 4 inputs IP67 standard addressing.
Connection to ASi bus via M12 5 m extension cable.
4 sensor inputs powered by the bus

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.E

I/O Configuration:
Inputs:
PNP type 24 VDC powered by the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	15
§%5	77
§%6	ASIMMO4I50
§%7	Mini-mod  4I std add M12-5
§%8	0.0.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XBL-C5012F581

Surface mountable keyboard - 12 keys
with tactile feedback for industrial applications.
Keys marking  : 0 to 9, + and -
Degree of protection  : IP65.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.F.F.F

I/O Configuration:
Inputs:
Key pressed: 0 1 2 3 4 5 6 7 8 9 + -     none
D0 --------> 0 1 0 1 0 1 0 1 0 1 0 1       1
D1 --------> 0 0 1 1 0 0 1 1 0 0 1 1       1
D2 --------> 0 0 0 0 1 1 1 1 0 0 0 0       1
D3 --------> 0 0 0 0 0 0 0 0 1 1 1 1       1
Hexadecimal: 0 1 2 3 4 5 6 7 8 9 A B       F

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	5
§%5	3
§%6	XBL-C5012F581
§%7	Surface mountable keyb 12 keys
§%8	0.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XBL-C5012R581

Flush mountable keyboard - 12 keys
with tactile feedback for industrial applications.
Keys marking  : 0 to 9, + and -
Degree of protection  : IP65.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.F.F.F

I/O Configuration:
Inputs:
Key pressed: 0 1 2 3 4 5 6 7 8 9 + -     none
D0 --------> 0 1 0 1 0 1 0 1 0 1 0 1       1
D1 --------> 0 0 1 1 0 0 1 1 0 0 1 1       1
D2 --------> 0 0 0 0 1 1 1 1 0 0 0 0       1
D3 --------> 0 0 0 0 0 0 0 0 1 1 1 1       1
Hexadecimal: 0 1 2 3 4 5 6 7 8 9 A B       F

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0:
P1:
P2:
P3:
§%3	f1
§%4	5
§%5	4
§%6	XBL-C5012R581
§%7	Flush mountable keyb 12 keys
§%8	0.F.F.F
§%9
§%10
§%11
§%12
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	APP1CAS2

TEGO POWER AS-Interface
This interface has 2 AS-Interf adresses which allow
up to 8 inputs and 8 outputs. The selection of the
informations is made by switches.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24V 5mA powered via the bus
D0: Status contactor/circuit breaker/local input
D1: Status contactor/circuit breaker/local input
D2: Status contactor/circuit breaker/local input
D3: Status contactor/circuit breaker/local input

Outputs:
24V 50 mA
D0: Control contactor coil / local output
D1: Control contactor coil / local output
D2: Control contactor coil / local output
D3: Control contactor coil / local output

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	51
§%6	APP1CAS2
§%7	ASi TEGO POWER interface 8I/8O
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASILUFC5

module TeSys model U
without sensor inputs
Operates with standard addressing

Version:

Supplier:	Telemecanique

AS-i Profil:	7.D.F.0

I/O Configuration:
Inputs:
D0:Not ready or fault=0 / Ready=1
D1: Stopped=0 / Running=1
D2: Reserved
D3: Reserved

Outputs:
D0: Stop=0 / Forward=1
D1: Stop=0 / Reverse=1
D2:Reserved
D3: Reserved

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	94
§%6	ASILUFC5
§%7	 AS-Interface TeSys model U
§%8	7.D.F.0
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29	16
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1#**D

Motor starter multi functions plastic case.
# = P rotary operator
# = M push button
** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Unused
D3: Unused

Outputs:
D0: Stop = 0 / Run = 1
D1: D0 and D1 = 1 : Reset
D2: Unused
D3: Unused

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	35
§%6	LF1#**D
§%7	Motor start. multi funct plas
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1#**DA78

Motor starter multi functions +2 sensors +1 actuator
plastic case.  # = P rotary operator
                      # = M push button
                      ** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Run = 1
D1: D0 and D1 = 1 : Reset
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	37
§%6	LF1#**DA78
§%7	Motor start mul fun +2s+1a pla
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1#**DA79

Motor starter multi func +2 sens + 1act + local/bus
plastic case.  # = P rotary operator
                      # = M push button
                      ** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Run = 1
D1: D0 and D1 = 1 : Reset
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	39
§%6	LF1#**DA79
§%7	Mot star m f +2s+1a+loc/bus pl
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1M#**D

Motor starter multi functions +2 sensors +1 actuator
metal case.  # = P rotary operator
                    # = M push button
                    ** = range

Version:

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Run = 1
D1: D0 and D1 = 1 : Reset
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	59
§%6	LF1M#**D
§%7	Motor start mul fun +2s+a met.
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1M#**DA79

Motor starter multi func +2 sens + 1act + local/bus
metal case.  # = P rotary operator
                    # = M push button
                     ** = range

Version:

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Run = 1
D1: D0 and D1 = 1 : Reset
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	60
§%6	LF1M#**DA79
§%7	Mot star m f +2s+1a+loc/bus me
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2#**D

Reversing motor starter multi function plastic case.
# = P rotary operator
# = M push button
** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Unused
D3: Unused

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2: Unused
D3: Unused
* D0 and D1 = 1 : Reset

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	36
§%6	LF2#**D
§%7	Rev. motor starter mul fun pla
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2#**DA78

Reversing motor starter mult functions +2sens +1act
plastic case  # = P rotary operator
                     # = M push button
                      ** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused
* D0 and D1 = 1 : Reset

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	38
§%6	LF2#**DA78
§%7	Rev mot start m f +2s +1a pla
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2#**DA79

Revers motor starter multi functions + 2sens+1 actu
+loc/bus plastic case # = P rotary operator
                                   # = M push button
                                   ** = range

Version:	1.1

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused
* D0 and D1 = 1 : Reset

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	40
§%6	LF2#**DA79
§%7	Re mot sta mf + 2s+1a+lo/bus p
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2M#**D

Reversing motor starter mult functions +2sens +1act
metal case   # = P rotary operator
                    # = M push button
                    ** = range

Version:

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused
* D0 and D1 = 1 : Reset

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	61
§%6	LF2M#**D
§%7	Rev mot start m f +2s +1a met
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2M#**DA79

Revers motor starter multi functions + 2sens+1 actu
+ loc/bus metal case  # = P rotary operator
                                   # = M push button
                                   ** = range

Version:

Supplier:	Telemecanique

AS-i Profil:	7.D.F.F

I/O Configuration:
Inputs:
D0: Not ready or fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2: Auxiliary output : Off = 0 / On = 1
D3: Unused
* D0 and D1 = 1 : Reset

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P1: Fall back position : Run = 0 / Stop = 1
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	62
§%6	LF2M#**DA79
§%7	Re mot sta mf + 2s+1a+lo/bus m
§%8	7.D.F.F
§%9	Watchdog
§%10	Fall back posit.
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF7P**D###§§§

Motor starter standard + 2 sensors
** = range
### = A74 with HARTING connectors
§§§ = A79 with local/bus selector switch

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:  Stopped = 1 / Running = 0
D1: Not ready or fault = 0 / Ready = 1
D2:  Sensor1 signal : No detection=0/Detection=1
D3:  Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Run = 1
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	56
§%6	LF7P**D###§§§
§%7	Motor starter standard +2 sens
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF8P**D###§§§

Reversing motor starter standard
** = range
### = A74 with HARTING connectors
§§§ = A79 with local/bus selector swith

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:  Stopped = 1 / Direct running = 0
D1: Stopped = 1 / Reversed running = 0
D2: Not ready or fault = 0 / Ready = 1
D3:

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	57
§%6	LF8P**D###§§§
§%7	Rev mot start standard
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF8P**DA78§§§

Reversing motor starter standard + 2 sensors
** = range
### = A74 with HARTING connectors
§§§ = A79 with local/bus selector swith

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0:  Stopped = 1 / Direct or reversed running = 0
D1: Not ready or fault = 0 / Ready = 1
D2: Sensor1 signal : No detection=0/Detection=1
D3: Sensor2 signal : No detection=0/Detection=1

Outputs:
D0: Stop = 0 / Forward = 1 *
D1: Stop = 0 / Reverse = 1 *
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	58
§%6	LF8P**DA78§§§
§%7	Rev mot start standard + 2sens
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI*R2E

module for 2 TEGO QUICKFIT power starters
Extended A/B addressing.  2 outputs control 2
contactors, the 4 inputs give the status of 2
contactors and 2 circuit breakers.  I.R. address

Version:

Supplier:	Telemecanique

AS-i Profil:	7.A.7.E

I/O Configuration:
Inputs:
D0: Contactor status starter 1
D1: Circuit breaker status starter 1
D2: Contactor status starter 2
D3: Circuit breaker status starter 2

Outputs:
D0: Control of contactor starter 1
D1: Control of contactor starter 2
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	84
§%6	ASI*R2E
§%7	TEGO QUICKFIT mod. 2 starters
§%8	7.A.7.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASI*R4

module for 4 TEGO QUICKFIT power starters
Standard addressing  4 outputs control 4
contactors, the 4 inputs give the status of 4
contactors. Infrared addressing.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.E

I/O Configuration:
Inputs:
D0: Contactor status starter 1
D1: Contactor status starter 2
D2: Contactor status starter 3
D3: Contactor status starter 4

Outputs:
D0: Control of contactor starter 1
D1: Control of contactor starter 2
D2: Control of contactor starter 3
D3: Control of contactor starter 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	85
§%6	ASI*R4
§%7	TEGO QUICKFIT mod. 4 starters
§%8	7.F.F.E
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LA9Z32810

2 inputs 1 output  interface for the control
of D.O.L. starters with LP1, LP4-K06 to K12
LP1-D09 to D32, and LP4-D09 to D25 contactors
Outputs 24VDC-0,5A solid-state

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
Powered via the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2:
D3:

Outputs:
Short circuits proof. Fallback = 0 by watchdog
D0:
D1:
D2: O-3 Output actuator 3
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	48
§%6	LA9Z32810
§%7	Motor inter. 2I/1O-24V 500 mA
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LA9Z32811

4 inputs 2 outputs  interface for the control
of D.O.L. starters with LP1, LP4-K06 to K12
LP1-D09 to D32, and LP4-D09 to D25 contactors
Outputs 24VDC-0,5A solid-state

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
Powered via the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Short circuits proof. Fallback = 0 by watchdog
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	4
§%5	49
§%6	LA9Z32811
§%7	Motor inter. 4I/2O-24V 500 mA
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1K09BW#**C

Previous version of direct motor starter.
Replaced by LF1#**D

Version:	1.2

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Unused
D1: Stopped = 0 / Running = 1
D2: Fault = 0 / OK = 1
D3: Not ready = 0 / Ready = 1

Outputs:
D0: Stop = 0 / Run = 1
D1: Unused
D2: Unused
D3: Unused

Parameters:
P0: Watchdog disable = 1 / Watchdog enable = 0
P1: Unused
P2: Normal mode = 1 / Reset mode = 0
P3: Default state : Stop = 1 / Run = 0
§%3	f1
§%4	4
§%5	20
§%6	LF1K09BW#**C
§%7	Direct motor starter mod. C
§%8	7.F.F.F
§%9	Watchdog
§%10	Unused
§%11	Reset
§%12	Default state
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF1K09BW#**CA78

Previous version of direct motor starter + 1 sensor.
Replaced by LF1#**DA78
at the end of the reference.

Version:	1.2

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Sensor signal
D1: Stopped = 0 / Running = 1
D2: Fault = 0 / OK = 1
D3: Not ready = 0 / Ready = 1

Outputs:
D0: Stop = 0 / Run = 1
D1: Unused
D2: Unused
D3: Unused

Parameters:
P0: Watchdog disable = 1 / Watchdog enable = 0
P1: Unused
P2: Normal mode = 1 / Reset mode = 0
P3: Default state : Stop = 1 / Run = 0
§%3	f1
§%4	4
§%5	21
§%6	LF1K09BW#**CA78
§%7	Direct motor starter + sens. C
§%8	7.F.F.F
§%9	Watchdog
§%10	Unused
§%11	Reset
§%12	Default state
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2K09BW#**C

Previous version of reversing motor starter.
Replaced by LF2#**D

Version:	1.2

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Unused
D1: Stopped = 0 / Running = 1
D2: Fault = 0 / OK = 1
D3: Not ready = 0 / Ready = 1

Outputs:
D0: Stop = 0 / Run = 1
D1: Forward = 0 / Reverse = 1
D2: Unused
D3: Unused

Parameters:
P0: Watchdog disable = 1 / Watchdog enable = 0
P1: Unused
P2: Normal mode = 1 / Reset mode = 0
P3: Default state : Stop = 1 / Run = 0
§%3	f1
§%4	4
§%5	22
§%6	LF2K09BW#**C
§%7	Reversing motor starter mod C
§%8	7.F.F.F
§%9	Watchdog
§%10	Unused
§%11	Reset
§%12	Default state
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	LF2K09BW#**CA78

Previous version of reversing motor starter+1 sensor
Replaced by LF2#**DA78
at the end of the reference.

Version:	1.2

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Sensor signal
D1: Stopped = 0 / Running = 1
D2: Fault = 0 / OK = 1
D3: Not ready = 0 / Ready = 1

Outputs:
D0: Stop = 0 / Run = 1
D1: Forward = 0 / Reverse = 1
D2: Unused
D3: Unused

Parameters:
P0: Watchdog disable = 1 / Watchdog enable = 0
P1: Unused
P2: Normal mode = 1 / Reset mode = 0
P3: Default state : Stop = 1 / Run = 0
§%3	f1
§%4	4
§%5	23
§%6	LF2K09BW#**CA78
§%7	Reversing motor start.+sens. C
§%8	7.F.F.F
§%9	Watchdog
§%10	Unused
§%11	Reset
§%12	Default state
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XUJ-K063539AS

Photo-electric detectors, compact type XUJ.
Polarised reflex system.
Range = 6 m.
Red transmission.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0: No object present = 0 / Object present = 1
D1: Weak reception: Alarm On =0 / Alarm Off = 1
D2: Unused
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Inversion of D0 =0 / No inversion of D0 = 1
P2: Unused
P3: Unused
§%3	f1
§%4	9
§%5	16
§%6	XUJ-K063539AS
§%7	Photo elect. detect. reflex
§%8	1.1.F.F
§%9	Unused
§%10	D0 inverted
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XUJ-K103534AS

Photo-electric detectors, compact type XUJ.
Thru-beam.
Range = 15 m.
Infra-red transmission.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0: No object present = 0 / Object present = 1
D1: Weak reception: Alarm On =0 / Alarm Off = 1
D2: Unused
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Inversion of D0 =0 / No inversion of D0 = 1
P2: Unused
P3: Unused
§%3	f1
§%4	9
§%5	15
§%6	XUJ-K103534AS
§%7	Photo elect. detect. Thru beam
§%8	1.1.F.F
§%9	Unused
§%10	D0 inverted
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XUJ-K123538AS

Photo-electric detectors, compact type XUJ
Diffuse with background suppression.
Range = 1,2  m.
Infra-red transmission.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0: No object present = 0 / Object present = 1
D1: Weak reception: Alarm On =0 / Alarm Off = 1
D2: Unused
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Inversion of D0 =0 / No inversion of D0 = 1
P2: Unused
P3: Unused
§%3	f1
§%4	9
§%5	18
§%6	XUJ-K123538AS
§%7	Photo elect. detect. bs.  1,2m
§%8	1.1.F.F
§%9	Unused
§%10	D0 inverted
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XUJ-K703538AS

Photo-electric detectors, compact type XUJ
Diffuse with background suppression.
Range = 0,7 m.
Infra-red transmission.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0: No object present = 0 / Object present = 1
D1: Weak reception: Alarm On =0 / Alarm Off = 1
D2: Unused
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Inversion of D0 =0 / No inversion of D0 = 1
P2: Unused
P3: Unused
§%3	f1
§%4	9
§%5	17
§%6	XUJ-K703538AS
§%7	Photo elect. detect. bs.  0,7m
§%8	1.1.F.F
§%9	Unused
§%10	D0 inverted
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	XUJ-ZAS1

Back over enables a conventional detector XUJ to be
connected to the AS-Interface bus.

Version:

Supplier:	Telemecanique

AS-i Profil:	1.1.F.F

I/O Configuration:
Inputs:
D0: No object present = 0 / Object present = 1
D1: Weak reception: Alarm On =0 / Alarm Off = 1
D2: Unused
D3:

Outputs:
D0:
D1:
D2:
D3: Unused

Parameters:
P0: Unused
P1: Inversion of D0 =0 / No inversion of D0 = 1
P2: Unused
P3: Unused
§%3	f1
§%4	9
§%5	19
§%6	XUJ-ZAS1
§%7	Back over for XUJ detectors
§%8	1.1.F.F
§%9	Unused
§%10	D0 inverted
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISSLB4

Safety interface for Harmony XB4 buttons
Connection to AS-Interface bus via IDC
Infrared programming

Version:

Supplier:	Telemecanique

AS-i Profil:	0.B.F.F

I/O Configuration:
Inputs:
D0: Table code
D1: Table code
D2: Table code
D3: Table code

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	16
§%5	68
§%6	ASISSLB4
§%7	Safety interface for XB4
§%8	0.B.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISSLB5

Safety interface for Harmony XB5 buttons
Connection to  AS-Interface bus via IDC
Infrared programming

Version:

Supplier:	Telemecanique

AS-i Profil:	0.B.F.F

I/O Configuration:
Inputs:
D0: Table code
D1: Table code
D2: Table code
D3: Table code

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	16
§%5	69
§%6	ASISSLB5
§%7	Safety interface for XB5
§%8	0.B.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISSLC1

Safety interface with 2 inputs on 1xM12.
Connection to  AS-Interface bus via IDC
Cable length connected to the M12 ports<3m max
Infrared programming

Version:

Supplier:	Telemecanique

AS-i Profil:	0.B.F.F

I/O Configuration:
Inputs:
D0: Table code
D1: Table code
D2: Table code
D3: Table code

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	16
§%5	71
§%6	ASISSLC1
§%7	Safety interface 2I on 1xM12
§%8	0.B.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISSLC2

Safety interface with 2 inputs on M12.
Connection to  AS-Interface bus via IDC
Cable length connected to the M12 ports<3m max
Infrared programming.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.B.F.F

I/O Configuration:
Inputs:
D0: Table code
D1: Table code
D2: Table code
D3: Table code

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	16
§%5	72
§%6	ASISSLC2
§%7	Safety interface 2I on M12
§%8	0.B.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISSLLS

Safety interface with 2 inputs on M16.
Connection to AS-Interface bus via IDC
Switch connected via M16.
Infrared programming

Version:

Supplier:	Telemecanique

AS-i Profil:	0.B.F.F

I/O Configuration:
Inputs:
D0: Table code
D1: Table code
D2: Table code
D3: Table code

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	16
§%5	70
§%6	ASISSLLS
§%7	Safety interface 2I on M16
§%8	0.B.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISAFEMON1

Safety monitor 1 channel
Relay output

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Diagnostic response code
D1: Diagnostic response code
D2: Diagnostic response code
D3: Diagnostic response code

Outputs:
D0: Diagnostic response code
D1: Diagnostic response code
D2: Diagnostic response code
D3: Diagnostic response code

Parameters:
P0:Unused
P1:Unused
P2:Unused
P3:Unused
§%3	f1
§%4	16
§%5	95
§%6	ASISAFEMON1
§%7	Safety monitor 1 channel
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ASISAFEMON2

Safety monitor 2 channels
Relay outputs

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
D0: Diagnostic response code
D1:  Diagnostic response code
D2: Diagnostic response code
D3: Diagnostic response code

Outputs:
D0: Diagnostic response code
D1: Diagnostic response code
D2: Diagnostic response code
D3: Diagnostic response code

Parameters:
P0:Unused
P1:Unused
P2:Unused
P3:Unused
§%3	f1
§%4	16
§%5	96
§%6	ASISAFEMON2
§%7	Safety monitor 2 channels
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8S40SB00

Telefast SB2  AS-Interface 4 inputs.
Used for the connection of 4 conventional sensors
on the AS-Interface bus. PNP Input 24Vdc.
Degree of protection  : IP20.

Version:

Supplier:	Telemecanique

AS-i Profil:	0.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc powered from the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	24
§%6	ABE-8S40SB00
§%7	4 I 24Vdc interface  IP20
§%8	0.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8S22SBB1

Telefast SB2  interface 2 inputs - 2 outputs.
For the connection of 2 conventional sensors and 2
actuators . Inputs PNP 24Vdc powered
via the bus . Outputs 24VDC-2A solid-state. IP20

Version:

Supplier:	Telemecanique

AS-i Profil:	3.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc powered via the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2:
D3:

Outputs:
Short circuits proof. Fallback = 0 by watchdog
D0:
D1:
D2: O-3 Solid-state output 24 V DC 2A Off = 0 / On = 1
D3: O-4 Solid-state output 24 V DC 2A Off = 0 / On = 1

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	46
§%6	ABE-8S22SBB1
§%7	2I/2O stat 2A interface IP20
§%8	3.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8S22SBB2

Telefast SB2 AS-Interface 2 inputs - 2 outputs.
For the connection of 2 conventional sensors and 2
actuators. Inputs PNP 24Vdc powered
via the bus Outputs 24VDC-2A solid state inver  IP20

Version:

Supplier:	Telemecanique

AS-i Profil:	3.F.F.F

I/O Configuration:
Inputs:
PNP 24Vdc powered via the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2:
D3:

Outputs:
Short circuits proof. Fallback = 1 by watchdog
D0:
D1:
D2: O-3 Solid-state output 24VDC 2A Off=1 / On=0
D3: O-4 Solid-state output 24VDC 2A Off=1 / On=0

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	54
§%6	ABE-8S22SBB2
§%7	2I/2O stat 2A interf IP20 inv.
§%8	3.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8R44SB11

Active user module.
Used for the connection of 4 sensors.
PNP Inputs
Maximum current for 4 sensors = 100 mA.

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP type
D0: I-1 Sensor signal 1 (pins 4-2)
D1: I-2 Sensor signal 2 (pins 4-2)
D2: I-3 Sensor signal 3 (pins 4-2)
D3: I-4 Sensor signal 4 (pins 4-2)

Outputs:
D0:
D1:
D2:
D3:

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	44
§%6	ABE-8R44SB11
§%7	User module 4 I 100 mA
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8S44SBB0

Telefast SB2  AS-Interface 4 inputs - 4 outputs.
Used for the connection of 4 conventional sensors
and 4 actuators . IP20  Isolated
inputs PNP 24VDC Outputs 24VDC-1A solid state

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc isolated from the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Outputs 24VDC-1A solid-state
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2: O-3 Output actuator 3
D3: O-4 Output actuator 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	26
§%6	ABE-8S44SBB0
§%7	4iI/4O sol sta 1A inter  IP20
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8S44SBB1

Telefast SB2  AS-Interface 4 inputs - 4 outputs
For the connection of 4 conventional sensors and 4
actuators on the AS-i bus. Inputs PNP 24Vdc powered
from the bus Outputs 24VDC-1A solid-state. IP20

Version:

Supplier:	Telemecanique

AS-i Profil:	7.0.F.F

I/O Configuration:
Inputs:
PNP 24Vdc powered from the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Outputs 24VDC-1A solid-state
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2: O-3 Output actuator 3
D3: O-4 Output actuator 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	43
§%6	ABE-8S44SBB1
§%7	4I/4O stat 1A interface  IP20
§%8	7.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8R44SF10

Telefast SB2  interface 4 inputs - 4 outputs.
For the connection of 4 conventional sensors and 4
actuators . Inputs 110V alt  isolated
from the bus Outputs relay EM 125V con/250V alt IP20

Version:

Supplier:	Telemecanique

AS-i Profil:	7.F.F.F

I/O Configuration:
Inputs:
110V alt isolated from the bus
D0: I-1 Sensor signal 1
D1: I-2 Sensor signal 2
D2: I-3 Sensor signal 3
D3: I-4 Sensor signal 4

Outputs:
Outputs relay EM 125V cont./250V alt - 5A
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2: O-3 Output actuator 3
D3: O-4 Output actuator 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	45
§%6	ABE-8R44SF10
§%7	4I 110V/4O relay interf  IP20
§%8	7.F.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	ABE-8R04S010

Telefast SB2  interface 4 outputs.
Used for the connection of 4 conventional actuators
 Relays outputs EM 125VDC / 250VAC-5A
Degree of protection  : IP20.

Version:

Supplier:	Telemecanique

AS-i Profil:	8.0.F.F

I/O Configuration:
Inputs:
D0:
D1:
D2:
D3:

Outputs:
Relays outputs EM 125VDC / 250VAC-5A
D0: O-1 Output actuator 1
D1: O-2 Output actuator 2
D2: O-3 Output actuator 3
D3: O-4 Output actuator 4

Parameters:
P0: Unused
P1: Unused
P2: Unused
P3: Unused
§%3	f1
§%4	12
§%5	25
§%6	ABE-8R04S010
§%7	4 O rel 250 V-5A interf.  IP20
§%8	8.0.F.F
§%9	Unused
§%10	Unused
§%11	Unused
§%12	Unused
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%2

Reference:	VW3A58305

Interface for variable speed controller ATV58
AS-Interface Profile :  7.E
Current consumption from AS-Interface bus : < 30 mA

Version:	1.0

Supplier:	Telemecanique

AS-i Profil:	7.E.F.F

I/O Configuration:
Inputs:
D0: Fault = 0 / Ready = 1
D1: Stopped = 0 / Running = 1
D2: LI3 off = 0 / LI3 on = 1
D3: If P3=0 : LI4 off = 0 / LI4 on =1
    If P3=1 : R2 off = 0 / R2 on =1

Outputs:
Bits D0 to D3 are encoded
Their signification depend on P1 and P2
They allow to control the stop mode,
the rotation sense, the speed, and the
RESET of the variable speed controller

Parameters:
P0: Watchdog : Disable = 0 / Enable = 1
P2 and P1: Mode select :
     00 : unused,    01 : +/- speed
     10 : 7 speeds,  11 : 4 speeds
P3: If 0 : D3 = LI4, if 1 D3 = R2
§%3	f1
§%4	13
§%5	47
§%6	VW3A58305
§%7	ASi interface for ATV58
§%8	7.E.F.F
§%9	Watchdog
§%10	Mode select
§%11	Mode select
§%12	Select input D3
§%13	1
§%14	1
§%15	1
§%16	1
§%17
§%18
§%19
§%20
§%21
§%22
§%23
§%24
§%25
§%26
§%27
§%28
§%29
§%30
§%31
§%32
§%33
§%34
§%35
§%36
§%37
§%38
§%39
§%40
§%41
§%42	f2
§%43	f3

